{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":43,"n_cols":13,"rows_kept":43,"cut":false,"hidden":false,"merged":[[2,0,2,1],[2,3,2,4],[0,0,1,4],[20,0,21,4],[22,0,22,1],[22,3,22,4],[20,7,21,11],[22,7,22,8],[22,10,22,11],[0,7,1,11],[2,7,2,8],[2,10,2,11],[24,12,30,12],[24,5,42,5],[3,5,18,5]]}
["上位机控制信号",{"$nulls":6},"上位机控制数字信号"]
[]
["上位机",null,"箭头","PLC",null,null,null,"上位机",null,"箭头","PLC"]
["名称","地址",null,"名称","地址","PLC常开信号输入",null,"名称","地址",null,"名称","地址"]
[null,null,"→","远程_45KW油泵启动","M2.0",{"$nulls":4},"→","45KW油路压力设定","VD108","浮点数输入"]
[null,null,"→","远程_45KW油泵停止","M2.1",{"$nulls":4},"→","15KW油路压力设定","VD112","浮点数输入"]
[null,null,"→","远程_15KW油泵启动","M2.2",{"$nulls":4},"→","冲洗压力设定","VD120","浮点数输入"]
[null,null,"→","远程_15KW油泵停止","M2.3",{"$nulls":4},"→","冲洗伸出时间设定","VW1004","整数"]
[null,null,"→","远程_循环泵启动","M2.4",{"$nulls":4},"→","冲洗缩回时间设定","VW1006","整数"]
[null,null,"→","远程_循环泵停止","M2.5",{"$nulls":4},"→"]
[null,null,"→","远程_45KW油路建压","M2.6"]
[null,null,"→","远程_45KW建压停止","M2.7"]
[null,null,"→","远程_15KW油路建压","M3.0"]
[null,null,"→","远程_15KW建压停止","M3.1"]
[null,null,"→","远程_A电磁阀启动","M3.2"]
[null,null,"→","远程_B电磁阀启动","M3.3"]
[null,null,"→","远程_防爆电磁阀1启动","M3.4"]
[null,null,"→","远程_防爆电磁阀2启动","M3.5"]
[null,null,"→","远程_远程软急停","M3.6"]
[]
["上位机显示信号",{"$nulls":6},"上位机显示数字信号"]
[]
["上位机",null,"箭头","PLC",null,null,null,"上位机",null,"箭头","PLC"]
["名称","地址",null,"名称","地址",null,null,"名称","地址",null,"名称","地址"]
[null,null,"←","远程_45KW电机运行信号","M5.0","PLC常开信号输出",null,null,null,"←","远程_A相电流","VD50","浮点数输出"]
[null,null,"←","远程_15KW电机运行信号","M5.1",{"$nulls":4},"←","远程_B相电流","VD54"]
[null,null,"←","远程_循环电机运行信号","M5.2",{"$nulls":4},"←","远程_C相电流","VD58"]
[null,null,"←","远程_45KW恒压运行信号","M5.3",{"$nulls":4},"←","远程_油箱温度","VD64"]
[null,null,"←","远程_15KW恒压运行信号","M5.4",{"$nulls":4},"←","远程_油箱液位","VD76"]
[null,null,"←","远程_备妥信号","M5.5",{"$nulls":4},"←","45KW油路压力","VD68"]
[null,null,"←","远程_45KW电机故障","M7.1",{"$nulls":4},"←","15KW油路压力","VD72"]
[null,null,"←","远程_15KW电机故障","M7.2"]
[null,null,"←","远程_回油油堵","M7.3"]
[null,null,"←","远程_进油油堵","M7.4"]
[null,null,"←","远程_循环油堵","M7.5"]
[null,null,"←","远程_15KW高压油堵","M7.6"]
[null,null,"←","远程_液位低于低限","M7.7"]
[null,null,"←","远程_温度高于高限","M8.0"]
[null,null,"←","远程_45KW压力高于高限","M8.1"]
[null,null,"←","远程_15KW压力高于高限","M8.2"]
[null,null,"←","远程_循环电机故障","M8.3"]
[null,null,"←","远程_45KW高压油堵","M8.4"]
[null,null,"←","远程_油站故障信号远传","M3.7"]