{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":95,"n_cols":10,"rows_kept":95,"cut":false,"hidden":false,"merged":[[1,1,2,3],[1,4,2,4]]}
[]
[null,"Modbus地址定义",null,null,"协议为Modbus TCP/IP\n默认端口502\n设备可以更改IP地址"]
[]
[null,"监视地址",{"$nulls":4},"监控地址"]
[null,"标准Modbus地址","数据类型","定义描述","备注说明",null,"标准Modbus地址","数据类型","定义描述","备注说明"]
[{"$nulls":6},42501,"BOOL","系统启动位","上升沿启动，会自动复位 （读写）"]
[{"$nulls":6},42501.1,"BOOL","系统停止位","上升沿停止，会自动复位 （读写）"]
[{"$nulls":6},42501.2,"BOOL","复位报警位","上升沿复位报警，会自动复位 （读写）"]
[]
[{"$nulls":6},42501.4,"BOOL","增益开关","打开=1，关闭=0 （读写）"]
[{"$nulls":6},42502,"INT","增益设置值","（0-100），（读写）"]
{"$rows_empty":12}
[{"$nulls":6},"水冷柜地址"]
[null,43012,"INT","系统运行状态","待机=0，报警=1 运行=2 （只读）",null,43061,"INT","系统运行状态","待机=0， 运行=1 报警=2（只读）"]
[null,43013,"INT","功放输出总电流","（4位数）只读",null,43063,"REAL","外循环压力"]
[null,43014,"INT","功放输出电压","（3位数）只读",null,43065,"REAL","动圈压力"]
[null,43015,"INT","励磁电流 ","（3位数）只读",null,43067,"REAL","励磁压力"]
[null,43016,"INT","励磁电压","（3位数）只读"]
[null,43017,"INT","三相电压","（3位数）只读",null,43071,"REAL","油泵压力"]
[null,43018,"INT","台体温度0","（3位数）只读",null,43073,"REAL","动圈流量"]
[null,43019,"INT","台体温度1","（3位数）只读",null,43075,"REAL","励磁流量"]
[null,43020,"INT","1柜直流电压","（3位数）只读",null,43077,"REAL","动圈供水温度"]
[null,43021,"INT","2柜直流电压","（3位数）只读",null,43079,"REAL","励磁供水温度"]
[null,43022,"INT","3柜直流电压","（3位数）只读"]
[null,43023,"INT","4柜直流电压","（3位数）只读",null,43083,"REAL","内部油泵温度"]
[]
[null,"报警位地址",{"$nulls":4},"报警位地址"]
[null,"标准Modbus地址","数据类型","定义描述","备注说明"]
[null,43051,"BOOL","门开关",null,null,43151.1,"BOOL","水冷柜热继报警"]
[null,43051.1,"BOOL","主柜热继",null,null,43151.199999999997,"BOOL","动圈水箱水位低"]
[null,43051.199999999997,"BOOL","冷却单元",null,null,43151.3,"BOOL","励磁水箱水位低"]
[null,43051.3,"BOOL","水平台油压",null,null,43151.4,"BOOL","油泵液位低"]
[null,43051.4,"BOOL","水平台过位移"]
[null,43051.5,"BOOL","台体导向静压轴承压力",null,null,43155,null,"外循环压力低"]
[null,43051.6,"BOOL","外部触发1",null,null,43155.199999999997,null,"动圈压力低"]
[null,43051.7,"BOOL","台体过位移",null,null,43155.4,null,"励磁压力低"]
[null,43051.8,"BOOL","台体温度",null,null,43155.8,null,"油泵压力低"]
[null,43051.9,"BOOL","变压器温度",null,null,43155.1,null,"动圈流量低"]
[null,43051.1,"BOOL","励磁控制继电器反馈",null,null,43155.12,null,"励磁流量低"]
[null,43051.11,"BOOL","冷却单元控制继电器反馈",null,null,43155.15,null,"动圈供水温度高"]
[null,43051.12,"BOOL","急停报警",null,null,43156.1,null,"励磁供水温度高"]
[null,43051.13,"BOOL","外部触发2",null,null,43156.5,null,"油泵温度高"]
[null,43051.14,"BOOL","柜1模块报警"]
[null,43051.15,"BOOL","柜2模块报警"]
[null,43051,"BOOL","柜1继电器反馈"]
[null,43052.1,"BOOL","柜2继电器反馈"]
[null,43052.2,"BOOL","外部急停1"]
[null,43052.3,"BOOL","外部变压器温度"]
[null,43052.4,"BOOL","柜3模块报警"]
[null,43052.5,"BOOL","柜4模块报警"]
[null,43052.6,"BOOL","柜3继电器反馈"]
[null,43052.7,"BOOL","柜4继电器反馈"]
[null,43104,"BOOL","输出电压报警"]
[null,43104.1,"BOOL","励磁欠流"]
[null,43104.2,"BOOL","励磁过流"]
[null,43104.3,"BOOL","励磁欠压"]
[null,43104.4,"BOOL","励磁过压"]
[null,43104.5,"BOOL","三相电压欠压"]
[null,43104.6,"BOOL","三相电压过压"]
[null,43104.7,"BOOL","柜1直流电压欠压"]
[null,43104.800000000003,"BOOL","柜1直流电压过压"]
[]
[null,43104.1,"BOOL","T01温度过高"]
[]
[null,43104.12,"BOOL","T00温度过高"]
[null,43104.13,"BOOL",null,"空"]
[null,43104.14,"BOOL","柜1输出电流过流"]
[null,43104.15,"BOOL","柜2直流电压欠压"]
[null,43105,"BOOL","柜2直流电压过压"]
[null,43105.1,"BOOL",null,"空"]
[null,43105.2,"BOOL","柜2输出电流过流"]
[null,43105.3,"BOOL",null,"空"]
[null,43105.4,"BOOL",null,"空"]
[null,43105.5,"BOOL",null,"空"]
[null,43105.599999999999,"BOOL",null,"空"]
[null,43105.7,"BOOL","柜3直流电压欠压"]
[null,43105.8,"BOOL","柜3直流电压过压"]
[null,43105.9,"BOOL","柜4直流电压欠压"]
[null,43105.1,"BOOL","柜4直流电压过压"]
[null,43105.11,"BOOL",null,"空"]
[null,43105.120000000003,"BOOL","柜3输出电流过流"]
[null,43105.13,"BOOL",null,"空"]
[null,43105.14,"BOOL","柜4输出电流过流"]
[null,43105.15,"BOOL"]