{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":32,"n_cols":15,"rows_kept":32,"cut":false,"hidden":false,"merged":[[0,0,0,2],[0,4,0,6],[0,8,0,10],[0,12,0,14]]}
["控制区(BOOL)",null,null,null,"控制区(Real)",null,null,null,"状态区(BOOL)",null,null,null,"控制区(Real)"]
["序号","地址","功能",null,"序号","地址","功能",null,"序号","地址","功能",null,"序号","地址","功能"]
[1,"DB1.DBX0.0","油泵1启动",null,1,"DB3.DBD0","压力控制1",null,1,"DB2.DBX0.0","油泵1运行中",null,1,"DB4.DBD0","实时液位"]
[2,"DB1.DBX0.1","油泵1停止",null,2,"DB3.DBD4",null,null,2,"DB2.DBX0.1","油泵1运行中",null,2,"DB4.DBD1","实时温度"]
[3,"DB1.DBX0.2","油泵2启动",null,3,"DB3.DBD8",null,null,3,"DB2.DBX0.2","冷却循环泵运行中",null,3,"DB4.DBD2","系统油压"]
[4,"DB1.DBX0.3","油泵2停止",null,4,"DB3.DBD12",null,null,4,"DB2.DBX0.3","软启1故障",null,4,"DB4.DBD3"]
[5,"DB1.DBX0.4","冷却循环泵启动",null,5,"DB3.DBD16",null,null,5,"DB2.DBX0.4","软启2故障",null,5,"DB4.DBD4"]
[6,"DB1.DBX0.5","冷却循环泵停止",null,6,"DB3.DBD20",null,null,6,"DB2.DBX0.5","冷却循环泵过载",null,6,"DB4.DBD5"]
[7,"DB1.DBX0.6",null,null,7,"DB3.DBD24",null,null,7,"DB2.DBX0.6",null,null,7,"DB4.DBD6"]
[8,"DB1.DBX0.7",null,null,8,"DB3.DBD28",null,null,8,"DB2.DBX0.7",null,null,8,"DB4.DBD7"]
[9,"DB1.DBX1.0",null,null,9,"DB3.DBD32",null,null,9,"DB2.DBX1.0",null,null,9,"DB4.DBD8"]
[10,"DB1.DBX1.1",null,null,10,"DB3.DBD36",null,null,10,"DB2.DBX1.1",null,null,10,"DB4.DBD9"]
[11,"DB1.DBX1.2",null,null,11,"DB3.DBD40",null,null,11,"DB2.DBX1.2",null,null,11,"DB4.DBD10"]
[12,"DB1.DBX1.3",null,null,12,"DB3.DBD44",null,null,12,"DB2.DBX1.3",null,null,12,"DB4.DBD11"]
[13,"DB1.DBX1.4",null,null,13,"DB3.DBD48",null,null,13,"DB2.DBX1.4",null,null,13,"DB4.DBD12"]
[14,"DB1.DBX1.5",null,null,14,"DB3.DBD52",null,null,14,"DB2.DBX1.5",null,null,14,"DB4.DBD13"]
[15,"DB1.DBX1.6",null,null,15,"DB3.DBD56",null,null,15,"DB2.DBX1.6",null,null,15,"DB4.DBD14"]
[16,"DB1.DBX1.7",null,null,16,"DB3.DBD60",null,null,16,"DB2.DBX1.7",null,null,16,"DB4.DBD15"]
[17,"DB1.DBX2.0",null,null,17,"DB3.DBD64",null,null,17,"DB2.DBX2.0",null,null,17,"DB4.DBD16"]
[18,"DB1.DBX2.1",null,null,18,"DB3.DBD68",null,null,18,"DB2.DBX2.1",null,null,18,"DB4.DBD17"]
[19,"DB1.DBX2.2",null,null,19,"DB3.DBD72",null,null,19,"DB2.DBX2.2",null,null,19,"DB4.DBD18"]
[20,"DB1.DBX2.3",null,null,20,"DB3.DBD76",null,null,20,"DB2.DBX2.3",null,null,20,"DB4.DBD19"]
[21,"DB1.DBX2.4",null,null,21,"DB3.DBD80",null,null,21,"DB2.DBX2.4",null,null,21,"DB4.DBD20"]
[22,"DB1.DBX2.5",null,null,22,"DB3.DBD84",null,null,22,"DB2.DBX2.5",null,null,22,"DB4.DBD21"]
[23,"DB1.DBX2.6",null,null,23,"DB3.DBD88",null,null,23,"DB2.DBX2.6",null,null,23,"DB4.DBD22"]
[24,"DB1.DBX2.7",null,null,24,"DB3.DBD92",null,null,24,"DB2.DBX2.7",null,null,24,"DB4.DBD23"]
[]
[]
[null,"液位保护(上下限)(停机限，报警限(80%))"]
[null,"油温保护(上限)(停机限，报警限(80%))"]
[null,"压力保护(上限)(停机限，报警限(80%))"]
[null,"滤油器报警(有几个滤油器就有几个报警信号)"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}