{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":31,"n_cols":13,"rows_kept":31,"cut":false,"hidden":false,"merged":[[17,12,22,12],[0,7,1,11],[2,7,2,8],[2,10,2,11],[17,5,30,5],[15,0,15,1],[15,3,15,4],[13,7,14,11],[15,7,15,8],[15,10,15,11],[2,0,2,1],[2,3,2,4],[0,0,1,4],[13,0,14,4],[4,5,11,5]]}
["上位机控制信号",{"$nulls":6},"上位机控制数字信号"]
[]
["上位机",null,"箭头","PLC",null,null,null,"上位机",null,"箭头","PLC"]
["名称","地址",null,"名称","地址",null,null,"名称","地址",null,"名称","地址"]
[null,null,"→","远程_油泵启动","M10.0","PLC常开信号输入",null,null,null,"→","系统压力设定值","VD500","浮点数输入"]
[null,null,"→","远程_油泵停止","M10.1",{"$nulls":4},"→","冲洗压力设定","VD1508","浮点数输入"]
[null,null,"→","远程_循环泵启动","M10.2",{"$nulls":4},"→","冲洗伸出时间","VW1504","整数"]
[null,null,"→","远程_循环泵停止","M10.3",{"$nulls":4},"→","冲洗缩回时间","VW1506","整数"]
[null,null,"→","远程_建压","M10.4",{"$nulls":4},"→"]
[null,null,"→","远程_泄压","M10.5",{"$nulls":4},"→"]
[null,null,"→","远程_冲洗启动","M5.0"]
[null,null,"→","远程_冲洗停止","M5.1"]
[]
["上位机显示信号",{"$nulls":6},"上位机显示数字信号"]
[]
["上位机",null,"箭头","PLC",null,null,null,"上位机",null,"箭头","PLC"]
["名称","地址",null,"名称","地址",null,null,"名称","地址",null,"名称","地址"]
[null,null,"←","远程_油泵运行正常信号","M20.0","PLC常开信号输出",null,null,null,"←","远程_A相电流","VD504","浮点数输出"]
[null,null,"←","远程_循环运行正常信号","M20.1",{"$nulls":4},"←","远程_B相电流","VD508"]
[null,null,"←","远程_油泵电机故障","M20.2",{"$nulls":4},"←","远程_C相电流","VD512"]
[null,null,"←","远程_循环泵电机故障","M20.3",{"$nulls":4},"←","远程_油箱温度","VD516"]
[null,null,"←","远程_回油堵塞信号1","M20.4",{"$nulls":4},"←","远程_油箱液位","VD520"]
[null,null,"←","远程_高压堵塞信号1","M20.5",{"$nulls":4},"←","远程_系统压力","VD524"]
[null,null,"←","远程_高压堵塞信号2","M20.6",{"$nulls":4},"←"]
[null,null,"←","远程备妥信号","M20.7",{"$nulls":4},"←"]
[null,null,"←","远程_急停信号","M21.0",{"$nulls":4},"←"]
[null,null,"←","远程_油箱温度上限到达","M21.1",{"$nulls":4},"←"]
[null,null,"←","远程_油箱液位下限到达","M21.2",{"$nulls":4},"←"]
[null,null,"←","远程_系统压力上限到达","M21.3",{"$nulls":4},"←"]
[null,null,"←","远程_故障报警","M21.4",{"$nulls":4},"←"]
[null,null,"←","远程_回油堵塞信号2","M21.5"]