{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["三向地震台","双向台","单向台","Stewart"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"三向地震台","index":0,"n_rows":15,"n_cols":15,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[{"$nulls":11},"有效面积/m²","流量L/min","缸单价/万元","阀单价"]
[null,null,"X最大速度m/s",1,"X最大加速度g",1,"台面及负载总质量t",10,null,"推力X/t",{"$f":"$H$2*1.5/2*F2","v":7.5},{"$f":"K2*9.8/14000","v":5.2500000000000003E-3},{"$f":"L2*D2*60000","v":315},{"$f":"IF(K2<5,5,IF(K2<10,6.5,IF(K2<20,9,IF(K2<30,11,IF(K2<50,16,20)))))","v":6.5},{"$f":"IF(M2<=60,2,IF(M2<=120,4,IF(M2<=250,19,IF(M2<=1000,24,46))))","v":24}]
[null,null,"Y最大速度m/s",1,"Y最大加速度",1,null,null,null,"推力Y",{"$f":"$H$2*1.5/2*F3","v":7.5},{"$f":"K3*9.8/14000","v":5.2500000000000003E-3},{"$f":"L3*D3*60000","v":315},{"$f":"IF(K3<5,5,IF(K3<10,6.5,IF(K3<20,9,IF(K3<30,11,IF(K3<50,16,20)))))","v":6.5},{"$f":"IF(M3<=60,2,IF(M3<=120,4,IF(M3<=250,19,IF(M3<=1000,24,46))))","v":24}]
[null,null,"Z最大速度m/s",1,"Z最大加速度",1,null,null,null,"推力Z",{"$f":"$H$2*1.5/4*F4","v":3.75},2.6250000000000002E-3,157.5,5,19]
[{"$nulls":9},"油源总流量L/min",{"$f":"(M2*2+M3*2+M4*4)*0.3","v":567}]
[]
[]
[]
[]
["缸总价/万元",{"$f":"N2*2+N3*2+N4*4","v":46}]
["油源总价/万元",{"$f":"IF(K5<=50,9,IF(K5<=200,20,CEILING((K5-200)/100,1)*7+20))","v":48}]
["控制系统/万元",25]
["阀总价/万元",{"$f":"O2*2+O3*2+O4*4","v":172}]
["机械部分总价/万元",0]
["五项成本价",{"$f":"SUM(B10:B14)","v":291}]

{"sheet":"双向台","index":1,"n_rows":15,"n_cols":15,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[{"$nulls":11},"有效面积/m²","流量L/min","缸单价/万元","阀单价"]
[null,null,"X最大速度m/s",1,"X最大加速度g",1,"台面及负载总质量t",10,null,"推力X/t",{"$f":"$H$2*1.5/2*F2","v":7.5},{"$f":"K2*9.8/14000","v":5.2500000000000003E-3},{"$f":"L2*D2*60000","v":315},{"$f":"IF(K2<5,5,IF(K2<10,6.5,IF(K2<20,9,IF(K2<30,11,IF(K2<50,16,20)))))","v":6.5},{"$f":"IF(M2<=60,2,IF(M2<=120,4,IF(M2<=250,19,IF(M2<=1000,24,46))))","v":24}]
[null,null,"Y最大速度m/s",1,"Y最大加速度",1,null,null,null,"推力Y",{"$f":"$H$2*1.5*F3","v":15},{"$f":"K3*9.8/14000","v":1.0500000000000001E-2},{"$f":"L3*D3*60000","v":630},{"$f":"IF(K3<5,5,IF(K3<10,6.5,IF(K3<20,9,IF(K3<30,11,IF(K3<50,16,20)))))","v":9},{"$f":"IF(M3<=60,2,IF(M3<=120,4,IF(M3<=250,19,IF(M3<=1000,24,46))))","v":24}]
[]
[{"$nulls":9},"油源总流量L/min",{"$f":"(M2*2+M3)*0.3","v":378}]
[]
[]
[]
[]
["缸总价/万元",{"$f":"N2*2+N3","v":22}]
["油源总价/万元",{"$f":"IF(K5<=50,9,IF(K5<=200,20,CEILING((K5-200)/100,1)*7+20))","v":34}]
["控制系统/万元",6]
["阀总价/万元",{"$f":"O2*2+O3","v":72}]
["机械部分总价/万元",0]
["五项成本价",{"$f":"SUM(B10:B14)","v":134}]

{"sheet":"单向台","index":2,"n_rows":15,"n_cols":15,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[{"$nulls":11},"有效面积/m²","流量L/min","缸单价/万元","阀单价"]
[{"$nulls":6},"台面及负载总质量t",10]
[]
[null,null,"Z最大速度m/s",1,"Z最大加速度/g",1,null,null,null,"推力Z",{"$f":"$H$2*1.5*F4","v":15},{"$f":"K4*9.8/14000","v":1.0500000000000001E-2},{"$f":"L4*D4*60000*0.8","v":504},{"$f":"IF(K4<5,5,IF(K4<10,6.5,IF(K4<20,9,IF(K4<30,11,IF(K4<50,16,20)))))","v":9},{"$f":"IF(M4<=60,2,IF(M4<=120,4,IF(M4<=250,19,IF(M4<=1000,24,46))))","v":24}]
[{"$nulls":9},"油源总流量L/min",{"$f":"M4*0.63","v":317.52}]
[]
[]
[]
[]
["缸总价/万元",{"$f":"N4","v":9}]
["油源总价/万元",{"$f":"IF(K5<=50,9,IF(K5<=200,20,CEILING((K5-200)/100,1)*7+20))","v":34}]
["控制系统/万元",5]
["阀总价/万元",{"$f":"O4","v":24}]
["机械部分总价/万元",0]
["五项成本价",{"$f":"SUM(B10:B14)","v":72}]

{"sheet":"Stewart","index":3,"n_rows":15,"n_cols":15,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
[{"$nulls":11},"有效面积/m²","流量L/min","缸单价/万元","阀单价"]
[{"$nulls":6},"台面及负载总质量t",15]
[]
[null,null,"Z最大速度m/s",1,"Z最大加速度/g",1.5,null,null,null,"推力Z",{"$f":"$H$2*1.5/6*F4","v":5.625},{"$f":"K4*9.8/14000","v":3.9375000000000009E-3},{"$f":"L4*D4*60000","v":236.25000000000006},{"$f":"IF(K4<5,5,IF(K4<10,6.5,IF(K4<20,9,IF(K4<30,11,IF(K4<50,16,20)))))","v":6.5},{"$f":"IF(M4<=60,2,IF(M4<=120,4,IF(M4<=250,19,IF(M4<=1000,24,46))))","v":19}]
[{"$nulls":9},"油源总流量L/min",{"$f":"M4*6","v":1417.5000000000005}]
[]
[]
[]
[]
["缸总价/万元",{"$f":"N4*6","v":39}]
["油源总价/万元",{"$f":"IF(K5<=50,9,IF(K5<=200,20,CEILING((K5-200)/100,1)*7+20))","v":111}]
["控制系统/万元",25]
["阀总价/万元",{"$f":"O4*6","v":114}]
["机械部分总价/万元",0]
["五项成本价",{"$f":"SUM(B10:B14)","v":289}]